Seapost 驾驶椅：Seapost只使用耐腐蚀性的硬件和双层金属饰面的外套,其中包括一个磷酸基外套,加上烤TGIC聚酯粉末涂料。这个可以达到1000小时的盐雾测试。

另外SeaPost提供适应人体工学的靠背，满足顾客的舒适度。

SeaPost use only non-corrosive hardware and a two-coat metal finish, which includes a phosphate base coat, plus a baked TGIC polyester powder paint. This finish can survive 1,000 hours of salt spray testing.

The SeaPost Helm offers complete adjustability and ergonomic support for ultimate occupant comfort.